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	C.O.S.H.H. ASSESSMENT

	Project/Contract/Location:
	Use:

	Substance/Trade Name: 
Portland Cement

	Supplier/Manufacturer (Name/Address/): 
Lafarge Cement UK

Portland House

Bickenhill Lane

Solihull

Birmingham

B37 7BQ

0845 8126232

	HAZARD (tick all that apply)
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	Explosive
	Flammable
	Oxidising
	Gas Under Pressure  
	Corrosive
	Acutely Toxic
	Health Hazard / Hazard to Ozone Layer
	Serious Health Hazard 
	Hazardous to the Environment

	
	
	
	
	
	
	
	
	

	Describe method of work (e.g. Sprayed/Brushed/Mixed etc.):

	Nature of product: 
Odourless White-Grey powder
	Where used (tick all that apply):

	
	OUTSIDE
	INSIDE

WELL VENTILATED
	INSIDE POORLY VENTILATED
	CONFINED SPACE

	Duration of use per day:
hrs
	
	
	
	

	Quantity used per day:


	
	
	
	

	Manufacturers Safety Data sheet available:  

YES
	MSDS revision:  
26.03.2012


	HANDLING / STORAGE / DISPOSAL PROCEDURE
	CONTROLS
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Bags should be stacked in a safe & stable manner in the dry.
Dispose of via an authorised waste contractor, observing all local & national regulations.
Store in a cool, dry and well-ventilated place.  Keep container closed when not in use. 

Powder form and cured form are not considered hazardous waste. 
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Clothing should be worn that prevents any Cement / Cement & water mixture coming into contact with the skin.
During pour, waterproof trousers & Wellingtons will be necessary.
Full Safety Goggles & safety gloves must be worn for all operations.  Wear FFP3 dust mask when mixing.  Do not breathe dust. 
Contaminated clothing should be removed & washed before use.

Wash hands and other exposed areas with mild soap before eating, drinking or smoking. 


	SPILLAGE / LEAKAGE PROCEDURE
	FIRE PROCEDURE
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Recover the spillage in a dry state if possible.
Minimise the generation of airborne dust.
The product can be slurried by the addition of water but will subsequently set as a hard material.
Keep children away from clear up.
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Cement is not flammable & will not facilitate combustion with other materials.
Use extinguishing media appropriate for surrounding fire. 

Do not use a heavy water stream.  Use of heavy stream of water may spread fire. 

	EMERGENCY MEDICAL PROCEDURES

	Eyes: 
Cautiously wash eyes immediately with plenty of clean water for at least 60 minutes & seek medical advice without delay.  Remove contact lenses if present and easy to do so. 
Corrosive to eyes. 


	Skin: 
Wash the affected area thoroughly with soap & water for at least 60 minutes.  Seek immediate medical advice.  Contaminated clothing should be removed & washed before use.
Corrosive to skin. 


	Ingestion: 
DO NOT induce vomiting.  Wash out mouth with water & drink plenty of water.  Seek medical advice immediately.  Never give anything by mouth to an unconscious person.  
May burn lining of mouth, throat and gastrointestinal tract. 


	Inhalation: 
If irritation occurs move to fresh air.  Keep warm and rest in a position comfortable for breathing.  If nose or airways become inflamed, or if other symptoms present, seek medical advice.
Corrosive to respiratory system. 


	HAZARD CLASSIFICATION

Irritant 
	PREPARED BY
	DATE/ISSUE

	

	C.O.S.H.H. ASSESSMENT


	 Substance: Portland Cement
	Ref: DGC_CA_01

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


	C.O.S.H.H. ASSESSMENT


	 Substance: Portland Cement
	Ref: HS_4.4_02

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


DGC_CA_01 Portland Cement                                                                                                                            April 2026
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