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	C.O.S.H.H. ASSESSMENT

	Project/Contract/Location:
	Use:

	Substance/Trade Name: 
Unleaded Petrol (Motor Spirits – Grades 95 & 98)
	Supplier/Manufacturer (Name/Address/): 
Total UK Ltd

40 Clarendon Road

Watford

Hertfordshire 
WD17 1TQ

01923 694000 / Emergency: 01923 427700

	HAZARD (tick all that apply)
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	Explosive
	Flammable
	Oxidising
	Gas Under Pressure  
	Corrosive
	Acutely Toxic
	Health Hazard / Hazard to Ozone Layer
	Serious Health Hazard 
	Hazardous to the Environment

	
	
	
	
	
	
	
	
	

	Describe method of work (e.g. Sprayed/Brushed/Mixed etc.):

	Nature of product: 
Light Yellow liquid with characteristic odour
	Where used (tick all that apply):

	
	OUTSIDE
	INSIDE

WELL VENTILATED
	INSIDE POORLY VENTILATED
	CONFINED SPACE

	Duration of use per day:
hrs
	
	
	
	

	Quantity used per day:


	
	
	
	

	Manufacturers Safety Data sheet available:  

YES 
	MSDS revision:  
26.09.2012


	HANDLING / STORAGE / DISPOSAL PROCEDURE
	CONTROLS
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Store packaged product (drums, cans etc.) in flammable away from water, moisture, heat, sparks, flames, static electricity & any source of ignition.  Store in designated containers.

DO NOT store exposed to the elements.
Waste should only be produced accidentally.
Excess should be recycled or burned.

Empty packaging may contain flammable or explosive vapours.  Packaging to be disposed of via licensed waste contractor to local regulations.
DO NOT cut, drill, grind or weld an empty container.
Avoid strong Oxidisers.
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Use in well ventilated area.
Wear safety gloves & glasses in case of splashing.
DO NOT smoke, eat or drink.
Avoid inhaling vapours & contact with the skin.
Remove contaminated clothing.
DO NOT SIPHON BY SUCKING WITH MOUTH
Keep away from food & beverages.
DO NOT use mobile phones.
Ensure product is poured slowly.

	SPILLAGE / LEAKAGE PROCEDURE
	FIRE PROCEDURE
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Cover discharged material with foam to reduce risk of ignition.
Contain & collect the spilt product with sand or any other inert absorbent material.
Preserve the waste in closed & sealed receptacles.
DO NOT allow penetration of sewers & watercourses.
DO NOT use dispersing agents.
Turn off all electrical supplies & prevent creation of sparks.
Vapours are heavier than air & may spread near ground level to sources of ignition.
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Use foam, CO2, powder, possible water spray extinguishers.
Use sand or earth for small fires. 

Solid water stream not to be used.
DO NOT simultaneously use water & foam extinguishers.
Cool tanks & surfaces exposed to fire with water spray.
Isolate the source of the combustible product & allow burning out under supervision or use appropriate extinguishers as applicable.
Fire fighters should use breathing apparatus.



	EMERGENCY MEDICAL PROCEDURES

	Eyes: 
Wash immediately with copious amounts of water, keeping eyelids apart for at least 15 minutes & consult a specialist.  Check for and remove any contact lenses. 
Eye contact may cause burning and redness. 

	Skin: 
Remove all soiled clothing, wash immediately & abundantly with soap & water.  Seek medical attention if irritation persists.  For minor burns, cool the skin under running water for at least 15 minutes.  If the product has been injected under the skin, transport to hospital immediately. 
Skin contact may cause irritation and redness. 

	Ingestion: 
DO NOT induce vomiting.  Do not give anything to drink.  Transfer to hospital immediately.  
May cause gastrointestinal irritation, nausea, vomiting, diarrhoea, and central nervous system depression.  

	Inhalation: 
In cases of exposure to intense concentration of vapours, fumes or spray, transport the person away from the contaminated zone.  Keep warm & allow to rest.  If the product is believed to have entered the lungs seek immediate medical attention.

May cause irritation of the respiratory tract, headache, nausea, vomiting, and altered state of consciousness. 

	HAZARD CLASSIFICATION

Flammable liquid
Aspiration Toxicity
Skin Irritant 
	PREPARED BY
	DATE/ISSUE

	

	C.O.S.H.H. ASSESSMENT


	 Substance: Unleaded Petrol (Motor Spirits – Grades 95 & 98) 
	Ref: ICP_CA_02

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	

	

	C.O.S.H.H. ASSESSMENT


	 Substance: Unleaded Petrol (Motor Spirits – Grades 95 & 98)
	Ref: DGC_CA_02

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


DGC_CA_02 Unleaded Petrol                                                                                                                            April 2026
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