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	C.O.S.H.H. ASSESSMENT

	Project/Contract/Location:
	Use: Fuelling diesel powered engines

	Substance/Trade Name: 
Gas Oil (Diesel)


	Supplier/Manufacturer (Name/Address/): 
Shell Trading International Limited
80 Strand

London

WC2R 0ZA
020 7546 2364 / Emergency: 0151 350 4595

Email: TRsds@shell.com

	HAZARD (tick all that apply)
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	Explosive
	Flammable
	Oxidising
	Gas Under Pressure  
	Corrosive
	Acutely Toxic
	Health Hazard / Hazard to Ozone Layer
	Serious Health Hazard 
	Hazardous to the Environment

	
	
	
	
	
	
	
	
	

	Describe method of work (e.g. Sprayed/Brushed/Mixed etc.):

	Nature of product: 
Yellow, Pale Straw or Red liquid with characteristic odour
	Where used (tick all that apply):

	
	OUTSIDE
	INSIDE

WELL VENTILATED
	INSIDE POORLY VENTILATED
	CONFINED SPACE

	Duration of use per day:
hrs
	
	
	
	

	Quantity used per day:


	
	
	
	

	Manufacturers Safety Data sheet available:  

YES
	MSDS revision:  
05.11.2012


	HANDLING / STORAGE / DISPOSAL PROCEDURE
	CONTROLS
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Store in a designated container or bunded tank away from sources of heat, sparks & ignition.
Avoid strong oxidising agents.

Suitable container materials are Steel, Aluminium, HDPE, PP, and FKM.
Partially filled containers present a greater hazard than those that are full.
Prevent ingress of water.
Dispose of waste to an authorised agent in accordance with local and national regulations.

EWC Code: 13 07 01 
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Use in well ventilated areas.  Avoid breathing vapours.
Avoid contact with skin.  Wash thoroughly after handling & immediately remove contaminated clothing & air dry prior to washing.  Wear chemical resistant gloves e.g. Nitrile or PVC, goggles, rubber boots e.g. wellingtons & chemical resistant apron should be worn if possibility of splashing.

DO NOT operate electrical equipment & remove all sources of ignition & naked flames when handling product
DO NOT smoke, eat or drink.  DO NOT siphon by mouth.
Ensure all equipment is earthed.
DO NOT cut, drill, grind or weld on or near containers.

	SPILLAGE / LEAKAGE PROCEDURE
	FIRE PROCEDURE
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Shut off leak & contain any spillage & absorb leak with suitable absorbent material (sand, earth) & transfer to a labelled sealable container, also remove any contaminated soil.
Remove all sources of ignition.
DO NOT flush away with water or allow to enter drains or watercourse.  Do not allow absorption into the ground. 
If spillage cannot be contained inform local authorities.

Air-dry contaminated clothing before washing.
Contaminated leather products e.g. shoes/boots cannot be decontaminated & should be disposed of as waste.

DO NOT breath fumes.
Vapour is heavier than air, beware of accumulation in pits & confined spaces.
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Use foam, water spray/fog.
Dry powder, CO2, earth/sand for small fires.  Water jet not to be used.
Thermal decomposition may produce toxic gases. 

Fire fighters should use self-contained breathing apparatus and protective clothing.
Keep containers cool by spraying with water.
Product will float on water & may re-ignite.

	EMERGENCY MEDICAL PROCEDURES

	Eyes: 
Flush eyes with copious quantities of water.  If irritation occurs obtain medical attention.

May cause irritation. 

	Skin: 
Remove contaminated clothing. Immediately flush skin with large amounts of water for at least 15 minutes, followed by washing with soap & water.  If symptoms occur seek medical attention. 
May cause redness, swelling, pain and blisters.

	Ingestion: 
DO NOT induce vomiting.  Seek medical attention.  If vomiting occurs spontaneously keep head below hips to prevent aspiration.  If within the next 6 hours a fever greater than 37oC, shortness of breath, chest congestion or continued coughing/wheezing appears seek immediate medical attention.

	Inhalation: 
Remove to fresh air.  If rapid recovery does not occur seek immediate medical attention.

High concentrations may cause dizziness, light-headedness, headache and nausea. 

	HAZARD CLASSIFICATION

Harmful 
	PREPARED BY
	DATE/ISSUE

	


	C.O.S.H.H. ASSESSMENT


	 Substance: Gas Oil (Diesel)


	Ref: DGC_CA_03 Gas Oil (Diesel)                                                                                                                             

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	C.O.S.H.H. ASSESSMENT


	 Substance: Gas Oil (Diesel)


	Ref: DGC_CA_03 Gas Oil (Diesel)                                                                                                                              

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


DGC_CA_03 Gas Oil (Diesel)                                                                                                                               April 2026 
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