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	C.O.S.H.H. ASSESSMENT

	Project/Contract/Location:
	Use:

	Substance/Trade Name: 
Sika 4a Waterstop
	Supplier/Manufacturer (Name/Address/): 
Sika Ltd.

Watchmead,

Welwyn Garden City

Hertfordshire

AL7 1BQ

01707 394444 / Emergency: 01707 363899

	HAZARD (tick all that apply)
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	Explosive
	Flammable
	Oxidising
	Gas Under Pressure  
	Corrosive
	Acutely Toxic
	Health Hazard / Hazard to Ozone Layer
	Serious Health Hazard 
	Hazardous to the Environment

	
	
	
	
	
	
	
	
	

	Describe method of work (e.g. Sprayed/Brushed/Mixed etc.):

	Nature of product: 

Odourless liquid, clear or straw colour
	Where used (tick all that apply):

	
	OUTSIDE
	INSIDE

WELL VENTILATED
	INSIDE POORLY VENTILATED
	CONFINED SPACE

	Duration of use per day:
hrs
	
	
	
	

	Quantity used per day:


	
	
	
	

	Manufacturers Safety Data sheet available:  

YES
	MSDS revision:  
30.09.2014


	HANDLING / STORAGE / DISPOSAL PROCEDURE
	CONTROLS
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Avoid contact with eyes, skin & clothing.
Exposure by inhalation or skin contact should be minimised by good industrial hygiene practices.
Keep in tightly closed original container, in cool dry area.
Avoid acids, halogenated compounds, Zinc, Brass & Aluminium.
Protect from frost.
Dispose as special waste in accordance with waste regulations by approved licensed waste contractor, this includes empty packaging.

EWC Code: 16 10 01 (product) / 15 01 10 (contaminated packaging)
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At all times wear tightly sealed chemical safety goggles, suitable rubber or PVC gloves (the inside of the gloves must be kept scrupulously clean).

Avoid contact with skin, eyes & clothing.
Ensure washing facilities and eye wash are available. 

Do not eat drink or smoke when using the product.  Wash hands after use, before breaks, and before eating, drinking, smoking or using the toilet. 


	SPILLAGE / LEAKAGE PROCEDURE
	FIRE PROCEDURE
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Wear appropriate protective clothing.
Prevent from entering watercourses or drains.  If pollution occurs, inform the relevant authorities. 
Absorb in inert material e.g. sand, earth, sawdust.

Scoop up material & place in suitable closed and labelled container for disposal.
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Use water spray or foam, or extinguishing media suitable for the surrounding environment. 
Fire fighters should wear self-contained breathing apparatus and full protective clothing.



	EMERGENCY MEDICAL PROCEDURES

	Eyes: 
Flush copiously with water for at least 15 minutes, ensuring thorough irrigation.  Obtain medical attention urgently.  Continue rinsing eyes during transport to hospital.  Remove contact lenses and keep eyes wide open while rinsing. 
Can cause severe eye damage and blindness. 

	Skin: 
Immediately wash with copious soap & water, rinse thoroughly & remove contaminated clothing as washing proceeds.  Obtain immediate medical attention.  Contaminated clothing must be washed or dry cleaned before re-use.
Can cause severe skin burns and dermatitis. 

	Ingestion: 
DO NOT induce vomiting.  Wash out mouth with water and afterwards drink plenty of water.  Obtain immediate medical attention.  Do not give milk or alcoholic beverages.  Never give anything by mouth to an unconscious person. 


	Inhalation: 
Remove from exposure to fresh air.  Keep warm & at rest.  Seek medical attention if victim feels unwell.

Irritating to respiratory system. 

	HAZARD CLASSIFICATION

Corrosive / Health Hazard 
	PREPARED BY
	DATE/ISSUE

	

	C.O.S.H.H. ASSESSMENT


	 Substance: Sika 4a Waterstop
	Ref: DGC_CA_04

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	C.O.S.H.H. ASSESSMENT


	 Substance: Sika 4a Waterstop
	Ref: DGC_CA_04

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


DGC_CA_04 Sika 4a Waterstop                                                                                                                         April 2026
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