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	C.O.S.H.H. ASSESSMENT

	Project/Contract/Location:
	Use: Sealant / Adhesive

	Substance/Trade Name: 
Sikaflex x-EBT
	Supplier/Manufacturer (Name/Address/):

Everbuild Building Products Ltd. 
Site 41, Knowsthorpe Way

Cross Green Industrial Estate

Leeds

LS9 0SW

Tel.: 0113 240 3456  

Email: sds@everbuild.co.uk

	HAZARD (tick all that apply)
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	Explosive
	Flammable
	Oxidising
	Gas Under Pressure  
	Corrosive
	Acutely Toxic
	Health Hazard / Hazard to Ozone Layer
	Serious Health Hazard 
	Hazardous to the Environment

	
	
	
	
	
	
	
	
	

	Describe method of work (e.g. Sprayed/Brushed/Mixed etc.): Applied using silicone gun

	Nature of product: 

Various coloured paste with characteristic odour
	Where used (tick all that apply):

	
	OUTSIDE
	INSIDE

WELL VENTILATED
	INSIDE POORLY VENTILATED
	CONFINED SPACE

	Duration of use per day:
4 hrs
	
	
	
	

	Quantity used per day:


	
	
	
	

	Manufacturers Safety Data sheet available:  

YES
	MSDS revision:  
11.03.2015


	HANDLING / STORAGE / DISPOSAL PROCEDURE
	CONTROLS
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Eating, drinking and smoking should be prohibited in areas where this material is handled, stored and processed. 
Wash hands and face before eating, drinking or smoking. 
Keep tightly closed when not in use.
Dispose of via a licensed waste disposal contractor. 

EWC Code: 08 04 10
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May cause eye irritation, skin irritation, irritation when inhaled, can cause gastrointestinal disturbances.

Avoid contact with eyes, skin and clothing.
Safety eyewear should be used.
Wash hands, forearms and face after handling chemical products.
Chemical resistant (nitrile) gloves should be worn at all times.

Personal protective equipment for the body should be selected, recommended use barrier skin cream.
Select respirator.



	SPILLAGE / LEAKAGE PROCEDURE
	FIRE PROCEDURE
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Avoid dispersal of split material and runoff and contact with soil, waterways, drains and sewers. 
Inform the relevant authorities if the product has caused environmental pollutions.
Absorb spill with an inert material and place in an appropriate waste disposal container.
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Use extinguishing measures that are appropriate to local circumstances and the surrounding environment. 

Use dry chemical, CO2, water spray or foam.  In a fire or if heated, a pressure increase will occur and the container may burst.
Firefighters should wear appropriate protective equipment and self-contained breathing apparatus.



	EMERGENCY MEDICAL PROCEDURES

	Eyes: 
Immediately flush eyes with plenty of water, keeping eye lids wide open.  Check for and remove any contact lenses.  Continue to rinse for at least 10 minutes.  Get medical attention.


	Skin: 
Flush contaminated skin with soap and plenty of water.  Remove contaminated clothing and shoes.  Get medical attention if symptoms occur.



	Ingestion: 
Clean mouth with water and drink plenty of water afterwards.  Do not induce vomiting unless directed to do so by medical personnel.  Maintain an open airway.  Seek immediate medical attention.


	Inhalation: 
Move to fresh air.  Get medical attention if symptoms occur.


	HAZARD CLASSIFICATION

Non-Hazardous
	PREPARED BY
	DATE/ISSUE

	

	C.O.S.H.H. ASSESSMENT


	 Substance: Sikaflex x-EBT
	Ref: DGC_CA_05

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	C.O.S.H.H. ASSESSMENT


	 Substance: Sikaflex x-EBT
	Ref: ICP_CA_05

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE
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