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	C.O.S.H.H. ASSESSMENT

	Project/Contract/Location:
	Use: Footing, walls, etc.

	Substance/Trade Name: 
Ready Mix Concrete
	Supplier/Manufacturer (Name/Address/): 
Breedon Aggregates Scotland Limited

Ethiebeaton Quarry
Kingennie,

Newbigging,

Angus

DD5 3RB

Tel.: (+44) 1382 537600

	HAZARD (tick all that apply)
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	Explosive
	Flammable
	Oxidising
	Gas Under Pressure  
	Corrosive
	Acutely Toxic
	Health Hazard / Hazard to Ozone Layer
	Serious Health Hazard 
	Hazardous to the Environment

	
	
	
	
	
	
	
	
	

	Describe method of work (e.g. Sprayed/Brushed/Mixed etc.): Use from concrete wagon

	Nature of product:

Grey granular paste no odour
	Where used (tick all that apply):

	
	OUTSIDE
	INSIDE

WELL VENTILATED
	INSIDE POORLY VENTILATED
	CONFINED SPACE

	Duration of use per day:
Hrs
	
	
	
	

	Quantity used per day:


	
	
	
	

	Manufacturers Safety Data sheet available:  

YES 
	MSDS revision:  
07.01.2015


	HANDLING / STORAGE / DISPOSAL PROCEDURE


	CONTROLS
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The hardening process of the concrete, mortar and screed can be delayed by the addition of additives and or admixtures.

Dispose of in accordance with local and national legal requirements.
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Direct skin contact with fresh concrete should be avoided.
Do not kneel or sit in wet materials.
Wear safety glasses, with long sleeved clothing, full length trousers, impervious gloves and impervious boots.



	SPILLAGE / LEAKAGE PROCEDURE
	FIRE PROCEDURE
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Prevent from entering drains, sewers or water courses.
Recover bulk spillage without delay and while material is still in a plastic state, using suction system or mechanical shovel.
The product can be slurried by the addition of water but will subsequently set as a hard material.
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 None

	EMERGENCY MEDICAL PROCEDURES

	Eyes: 
Immediately and thoroughly irrigate with water.

Wet material can cause irritation, inflammation or burns on contact with the eyes. 

	Skin: 
Where skin contact occurs with concrete, mortar and screed, either directly or through saturated clothing, the concrete must be washed off immediately with soap and water.  Where concrete enters boots or gloves or saturates clothing the article should be removed immediately and washed before further use.
Can cause irritation, dermatitis, burns, skin ulceration, and skin disease.  May cause severe burns without pain being felt. 



	Ingestion: 
Wash out mouth and drink plenty of water. Do not induce vomiting. Seek medical advice if a large amount is swallowed.
Ingestion of large amounts may cause stomach and intestine irritation.

	Inhalation: 
If irritation occurs, move to fresh air. If nose or airways become inflamed seek medical advice.
Inhalation of dust may cause lung damage and can be fatal.  

	HAZARD CLASSIFICATION

Irritant 
	PREPARED BY
	DATE/ISSUE

	

	C.O.S.H.H. ASSESSMENT


	 Substance: Ready Mix Concrete
	Ref: DGC_CA_06

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	C.O.S.H.H. ASSESSMENT


	 Substance: Ready Mix Concrete
	Ref: DGC_CA_06

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE
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