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	C.O.S.H.H. ASSESSMENT

	Project/Contract/Location:
	Use: For 2 stroke machines

	Substance/Trade Name: 
Universal Two Stroke Oil
	Supplier/Manufacturer (Name/Address/): 
Pennine Lubricants

Unit 35, Nutwood Trading Estate,

Limestone Cottage Lane,

Sheffield

S6 1NL

Tel.: 0114 285 2987

	HAZARD (tick all that apply)
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	Explosive
	Flammable
	Oxidising
	Gas Under Pressure  
	Corrosive
	Acutely Toxic
	Health Hazard / Hazard to Ozone Layer
	Serious Health Hazard 
	Hazardous to the Environment

	
	
	
	
	
	
	
	
	

	Describe method of work (e.g. Sprayed/Brushed/Mixed etc.): Poured into mixing can

	Nature of product: 
Viscous blue-green liquid with characteristic odour
	Where used (tick all that apply):

	
	OUTSIDE
	INSIDE

WELL VENTILATED
	INSIDE POORLY VENTILATED
	CONFINED SPACE

	Duration of use per day:
Hrs
	
	
	
	

	Quantity used per day:


	
	
	
	

	Manufacturers Safety Data sheet available:  

YES
	MSDS revision:  
20.07.2016


	HANDLING / STORAGE / DISPOSAL PROCEDURE
	CONTROLS
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Store in dry conditions between 0 and 40°C.
Store in a cool, well-ventilated area. 

Keep container tightly closed. 

Keep away from strong acids and strong oxidising agents. 
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Wear oil impervious gloves in cases of prolonged or repeated skin contact. 
Change heavily contaminated clothing and overalls as soon as possible.
Safety glasses should be worn.

Ensure eye bath is to hand.

Wear protective clothing and do not allow exposed skin. 

	SPILLAGE / LEAKAGE PROCEDURE
	FIRE PROCEDURE

	[image: image12.png]


 
Small spills: soak in absorbent granules or sand.
Large spills: Bund using absorbent granules, sand or earth and reclaim bulk liquid.
Transfer to a closable, labelled salvage container for disposal by an appropriate method. 

Prevent spills from entering drains/water courses.
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May support combustion in a serious fire.
Use suitable extinguishing media for the surrounding fire.

Extinguish with foam, dry powder, CO2, sand or earth.
Use water spray to cool containers.
In combustion emits toxic fumes.

Fire fighters should wear self-contained breathing apparatus and protective clothing to prevent contact with skin and eyes.  

	EMERGENCY MEDICAL PROCEDURES

	Eyes: 
Immediately wash eye thoroughly with plenty of clean water.  Bathe eye for at least 15 minutes. 
Contact with the eyes may cause irritation and redness. 

	Skin: 
Wash skin immediately and thoroughly with soap and water.  Remove heavily contaminated clothing.  Wash contaminated clothing before re-use.  If irritation persists, obtain medical advice.
There may be mild irritation at the site of contact. 

	Ingestion: 
Do not induce vomiting.  Wash out mouth with water and obtain medical attention.
Ingestion may cause irritation of the throat. 

	Inhalation: 
Not expected to be a problem.  Consult a doctor if any irritation occurs.  

	HAZARD CLASSIFICATION

Non-Hazardous 
	PREPARED BY
	DATE/ISSUE

	

	C.O.S.H.H. ASSESSMENT


	 Substance: Universal Two Stroke Oil
	Ref: DGC_CA_07

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	C.O.S.H.H. ASSESSMENT


	 Substance: Universal Two Stroke Oil
	Ref: DGC_CA_07

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE
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