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	C.O.S.H.H. ASSESSMENT

	Project/Contract/Location:
	Use: Lubricating grease

	Substance/Trade Name: 
Lithium Grease
	Supplier/Manufacturer (Name/Address/): 
Pennine Lubricants

Unit 35, Nutwood Trading Estate

Limestone Cottage Lane

Sheffield 
S6 1NL

Tel: 0114 285 2987

	HAZARD (tick all that apply)
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	Explosive
	Flammable
	Oxidising
	Gas Under Pressure  
	Corrosive
	Acutely Toxic
	Health Hazard / Hazard to Ozone Layer
	Serious Health Hazard 
	Hazardous to the Environment

	
	
	
	
	
	
	
	
	

	Describe method of work (e.g. Sprayed/Brushed/Mixed etc.):

	Nature of product:

Brown paste with characteristic odour
	Where used (tick all that apply):

	
	OUTSIDE
	INSIDE

WELL VENTILATED
	INSIDE POORLY VENTILATED
	CONFINED SPACE

	Duration of use per day:
Hrs
	
	
	
	

	Quantity used per day:


	
	
	
	

	Manufacturers Safety Data sheet available:  

YES
	MSDS revision:  
18.09.2012


	HANDLING / STORAGE / DISPOSAL PROCEDURE
	CONTROLS
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Store in dry conditions between 0oC and 40oC degree.
Avoid heat and Strong oxidising agents. 
	[image: image11.jpg]


 
If eye contact is possible, safety glass with side shields or goggles must be worn.
Ensure eye bath is available. 

If prolonged or repeated skin contact is likely, oil impervious gloves must be worn.
Protective clothing should be worn to keep the skin covered. 

	SPILLAGE / LEAKAGE PROCEDURE
	FIRE PROCEDURE
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Always prevent entry into drains or watercourses.
Spillage can be slippery.
Small spills – Gather into containers and dispose of as waste.
Large spills – Bund using absorbent granules, sand or earth and reclaim bulk product.
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Use CO2, foam, dry chemical or water fog to extinguish.
Use water to keep fire exposed containers cool.
Water spray may be used to flush spills away from exposures.
Prevent run-off from fire control from entering waterways or drinking water.
Product emits toxic fumes in combustion. 

Fire fighters to wear self contained breathing apparatus and protective clothing.



	EMERGENCY MEDICAL PROCEDURES

	Eyes: 
Flush thoroughly with water for 15 minutes.  If irritation occurs seek medical advice.

Contact with the eyes may cause irritation and redness. 

	Skin: 
Wash contact areas immediately with soap and water.  High pressure accidental injection through the skin requires immediate medical attention for possible incision, irrigation & or debridement (removal of infected tissue).
Skin contact may cause mild irritation. 


	Ingestion: 
Do not induce vomiting.  Wash out mouth with water and obtain medical attention.  Treat symptomatically.  If aspiration is suspected, obtain immediate medical attention.
There may be irritation of the throat. 



	Inhalation: 
Not expected to be a problem.
There may be irritation of the throat with a feeling of tightness in the chest. 


	HAZARD CLASSIFICATION

Non-Hazardous
	PREPARED BY
	DATE/ISSUE

	

	C.O.S.H.H. ASSESSMENT


	 Substance: Lithium Grease 
	Ref: DGC_CA_07

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	C.O.S.H.H. ASSESSMENT


	 Substance: Lithium Grease
	Ref: DGC_CA_07

	I have read, understood and agreed to work in accordance with the above control measures.

	NAME
	SIGN
	DATE
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