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	HEALTH & SAFETY RISK ASSESSMENT 

	Activity:
	Installation of Manhole Rings
	Site:
	
	Ref No:
	DGC_RA_0006

	Completed by:
	
	Position:
	Director
	Signed:
	
	Date:
	

	Who may be affected (Number of People?)

	Directly Affected:
	Employee
	3
	Subcontractors
	1
	Official visitors
	0
	General public
	0
	Indirectly Affected
	6

	Initial Risk
Before control measures are put in place
	Control Measures
	Residual Risk

After control measures are put in place

	No
	Hazards 
	L
	X
	S
	Score
	H/M/L
	Description
	L
	X
	S
	Score
	H/M/L

	1
	Falling Objects
	3
	X
	3
	9
	H
	1. Excavators Used for Lifting ICP RA 0050 controls must be applied when lifting manhole rings.
2. Work area to be barriered off from other work activities.

3. Operatives must not at any time place themselves in a potential trap situation between the load being lifted and any other object. (manhole box, vehicle item of equipment).

4. All operatives to stay out of swing area which the rings are being lifted in/out of position.  Banksman to attend all times. 
	2
	X

	1
	2
	L

	2
	Concrete
	3
	X
	3
	9
	H
	1. Suitable level concrete base to be in place prior to lowering manhole ring into excavation. 

2. When placing, handling & pouring wet Concrete PVC safety gloves, safety Wellington boots, safety goggles/glasses & waterproof over trousers to be worn. 

3. All Concrete splashes to skin to be washed off immediately & any contaminated clothing removed.

	2

	X
	1
	2
	L

	3
	Collapse of Excavation
	3
	X
	3
	9
	H
	All excavations to be stepped/battered back to the angle of repose prior to anyone gaining access into the excavation. Suitable tied/fixed ladder to be in place to gain access safely.
1. If excavation must be shored, then a temporary works design must be completed by a temporary works designer prior to any works commencing. 
2. Manhole boxes are to be utilised to prevent collapse of excavation. Manhole shutters must be in good condition before use. Chains must be connected to the correct lifting points when lifting them in/out of the excavation. If lifting point are bent/damaged do not use. Ensure there are no sharp edges around the perimeter of the shutters. 

3. Stop blocks or berm to be put in place to prevent vehicles surcharging the excavation.

	2

	X
	1
	2
	L

	4
	Plant Movement
	3
	X
	3
	9
	H
	1. All plant operators must hold current certification/tickets to operate the item of plant they have been trained to use. Under no circumstances must anyone operate any item of plant they do not hold a current certificate/ticket for.
2. Daily plant inspection must be carried out by the operator and signed off by the Site Manager prior to any use of plant.  This must be done each day. 

3. Adequate plant/pedestrian segregation MUST be in place as per company standards.
	1

	X
	1
	1
	L

	5
	Access/Egress
	3
	X
	2
	6
	M
	1. Suitable ladder access must be used to gain access/egress to work areas, including inside the manhole ring e.g. Benching base of manhole.
2. Manhole covers are only to be lifted by mechanical means or by using the correct manhole cover lifting handles.  If manually lifting manhole covers the Risk Assessment for Manually lifting Manhole Covers must be read, signed, understood and fully complied with. 
	2

	X
	1
	2
	L

	6
	Lifting Equipment Failure
	3
	X
	3
	9
	H
	1. All lifting equipment must have current certification & be colour coded with the current colour code.

2. The chains must be at the correct angle when lifting the manhole ring ideally 900. 

3. The correct sized chains (length & WLL) must be used for the lifting the manhole rings, lifting points must be checked prior to any lifting operation. Manhole ring lifters must then be inserted into the holes on the rings, and the chains must be hooked on inside the ring to prevent damage to the ring and reduce the angle of the lift. 

4. Trial lifts to be undertaken prior to lift.
	1
	X
	1
	1
	L

	7
	Falls From Height
	3
	X
	3
	9
	H
	Edge protection to be erected around all excavations. 
	1
	X
	1
	1
	L

	8
	Noise/Dust
	3
	X
	3
	9
	H
	M rated Dust suppression/Extraction to be used for any cutting and FFP3 dust mask and ear defenders to be always worn.
	2
	X
	1
	2
	L

	9
	Confined Space
	3
	X
	3
	9
	H
	Only trained and competent persons are permitted to enter confined spaces. 
	1
	X
	1
	1
	L

	10
	Manual Handling 
	3
	X
	3
	9
	H
	Mechanical aides will be used for all lifting. All lifts to be always kept inside the site boundary.
	1
	X
	1
	1
	L

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Refer to Toolbox Talks DA_TBT_220, DA_TBT_197, DA_TBT_198, DA_TBT_223, DA_TBT_172, DA_TBT_296
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	MANDATORY PPE – Hard hat, High-viz vest, Safety boots with steel toe and mid-sole 
	
	
	
	
	

	
	
	
	
	
	
	
	ADDITIONAL PPE REQUIRED – Ear Defenders, FFP3 Dust Mask
	
	
	
	
	

	Likelihood (L)
	Severity (S)
	Score (Likelihood x Severity) (LXS)
	Rating

	1 = Improbable
	1 = Minor
	7 - 9
	High

	2 = Probable
	2 = Moderate
	4 – 6
	Medium

	3 = Certain
	3 = Serious Injury
	1 - 3
	Low
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	Certain
	4-6
	7-9
	7-9
	
	H
	High Risk
	Additional control measures required to reduce the residual risk to an acceptable level. A full method statement must be provided with this risk assessment. Both must be communicated to all persons involved with the task prior to the commencement of the task.

	
	Probable
	1-3
	4-6
	7-9
	
	M
	Medium Risk
	Ensure that identified control measures are adequate. Are there further control measures which could be implemented to lower the risk?

	
	Improbable
	1-3
	1-3
	4-6
	
	L
	Low Risk
	Proceed with task having implemented all identified controls

	
	
	Minor
	Moderate
	Serious Injury
	
	NOTE: Prior to the commencement of works any new Risk Assessments that have been prepared on site must be sent to the H&S Department for review and uploading on the shared drive.

	

	Photographs

	

	Key Points / Good Practice

	

	

	

	

	

	On each site and each location, the generic assessment below must be reviewed to ensure that all significant hazards and their risks are identified and controlled.  Please fill in the number of people who are directly affected.

This side of the Assessment must be filled in to make the Risk Assessment site specific.

	SITE / LOCATION: 
ACTIVITY:

Installation of Manhole Rings
ADDITIONAL SPECIFIC HAZARDS:

ADDITIONAL CONTROL MEASURES:

ASSESSMENT OF REMAINING RISKS:   Low /Medium / High
	EMERGENCY PROCEDURES

ARE EMERGENCY PROCEDURES REQUIRED FOR THIS OPERATION: Yes  /  No

Name of competent person(s) appointed to take action.

TICK WHICH MAY REQUIRE ADDITIONAL ASSESSMENT TO BE DONE.

MANUAL

HANDLING

NOISE

COSHH

Method

Statement

OTHER

CIRCULATION OF RISK ASSESSMENT:

Tick Box

Contact and Emergency Numbers
Safety Department 

Site File
Brief operatives on assessments 
Revision

ON-SITE ASSESSMENT SIGNED:                                                        Date:

POSITION:


	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Installation of Manhole Rings
	Ref: DGC_RA_0006

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Installation of Manhole Rings
	Ref: DGC_RA_0006

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Installation of Manhole Rings
	Ref: DGC_RA_0006

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:


Likelihood





Severity
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