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	HEALTH & SAFETY RISK ASSESSMENT

	Activity:
	Operating a Dumper  
	Site:
	
	Ref No:
	DGC_RA_0010

	Completed by:
	
	Position:
	Director
	Signed:
	
	Date:
	

	Who may be affected (Number of People?)

	Directly Affected:
	Employee
	4
	Subcontractors
	2
	Official visitors
	0
	General public
	0
	Indirectly Affected
	12

	Initial Risk
Before control measures are put in place
	Control Measures
	Residual Risk

After control measures are put in place

	No
	Hazards 
	L
	X
	S
	Score
	H/M/L
	Description
	L
	X
	S
	Score
	H/M/L

	1
	Vehicle Operation 
	3
	X
	3
	9
	H
	1. Only qualified and authorised operators are to operate dumpers, NPORS/CPCS certified.
2. Daily inspections must be carried out prior to operating the dumper and these must be recorded using plant defect sheets. 

3. Any faults of damage must be reported to the Site Manager immediately. Do not operate if any faults are found. 

4. No persons under 18 years old are permitted to operate a dumper. 

5. Be aware of the terrain to be traversed & take appropriate action as required e.g. in wet or icy conditions, or on slippery gradients.

6. Never drive on gradients steeper than 1 in 4 (25%). Always travel up gradients with the load facing up hill. Always reverse down a gradient when loaded. Never attempt to run on or drive across a gradient. Avoid parking the machine on gradients. Choose a route to avoid gradients. 

7. Drives must wear their seat belt. Passengers must not be carried. 

8. All dumpers must be fitted with Roll Over Protection Systems (ROPS) & seat belts must be fitted & used. 

9. Site Manager to ensure speed restrictions are enforced & monitor use on slopping ground.   5mph
	1
	X
	1
	1
	L

	2
	Vehicle falling into excavations
	3
	X
	3
	9
	H
	1. Dumper skips are to be kept clean, to facilitate unloading free flowing materials. 
2. Operators must read and understand the site traffic management system and be aware of changes as required due to ongoing works.   
3. Stop boards are required at excavation sides where dumpers are working.
	1
	X
	1
	1
	L

	3
	Noise & emissions from vehicles
	3
	X
	2
	6
	M
	1. Adequate ventilation required for operation in confined spaces. (within Buildings). 

2. Vehicles must be checked by drivers before use, secured afterwards & must be operated in accordance with the manufacturer’s instructions.
	1
	X
	1
	1
	L

	4
	Injury to pedestrians/operatives
	3
	X
	3
	9
	H
	1. Even loading of dumpers to be achieved, no projecting materials. 

2. Lighting required for work in poor visibility. 

3. Public & operatives’ access to vehicle routes should be limited where practicable.
	1
	X
	1
	1
	L

	5
	Persons falling from vehicle
	3
	X
	1
	3
	L
	During loading driver to dismount from the dumper. When dismounting use three points of contact & descend backwards.
	1
	X
	1
	1
	L

	6
	Plant Movement 
	3
	X
	3
	9
	H
	1. Dumpers are not to be left unattended with engines running, keys must be removed. 

2. Handbrake to be applied when loading, tipping or parked (keys to be removed when left unattended). 

3. A Banksman is to be used where drivers’ vision is impaired or operating in congested areas. 

4. Keep to designated vehicle routes. 

5. Use correct towing pins. Do not use bent pieces of rebar as a towing pin. 

6. Vehicles must not be driven at excessive speeds & only in accordance with site conditions. 

7. Drivers must be competent & authorised to drive the type of vehicle. Driver training to CPCS standard or equivalent is required. 

8. Dumper driving by unauthorised operatives is not permitted: this also applies to subcontractors.
	2
	X
	1
	2
	L

	7
	Equipment Failure 
	2
	X
	2
	4
	M
	Planned maintenance programme applies to all dumpers & the Operators plant inspection log for the dumper is to be filled out daily following inspection of the dumper. Tyres are to be regularly checked (pressure gauge held on site) along with daily checks of the brakes, steering & hydraulics etc.
	1
	X
	1
	1
	L

	8
	Plant/pedestrian segregation
	3
	X
	3
	9
	H
	Ensure haul routes are well segregated from pedestrian walkways, only used approved haul routes.
	1
	X
	1
	1
	L

	
	
	
	
	
	
	
	Refer to Toolbox Talks CITB_B09, CITB_C07, CITB_C09, CITB_C16, CITB_C17, CITB_C21, CITB_D10, CITB_F02, HS_9.9_04, HS_9.9_06, HS_9.9_09, HS_9.9_30, HS_9.9_39
	
	
	
	
	

	
	
	
	
	
	
	
	MANDATORY PPE – Hard hat, High-viz vest, Safety boots with steel toe and mid-sole 
	
	
	
	
	

	
	
	
	
	
	
	
	ADDITIONAL PPE REQUIRED – 
	
	
	
	
	

	Likelihood (L)
	Severity (S)
	Score (Likelihood x Severity) (LXS)
	Rating

	1 = Improbable
	1 = Minor
	7 - 9
	High

	2 = Probable
	2 = Moderate
	4 – 6
	Medium

	3 = Certain
	3 = Serious Injury
	1 - 3
	Low

	[image: image1][image: image2.png]



	Certain
	4-6
	7-9
	7-9
	
	H
	High Risk
	Additional control measures required to reduce the residual risk to an acceptable level. A full method statement must be provided with this risk assessment. Both must be communicated to all persons involved with the task prior to the commencement of the task.

	
	Probable
	1-3
	4-6
	7-9
	
	M
	Medium Risk
	Ensure that identified control measures are adequate. Are there further control measures which could be implemented to lower the risk?

	
	Improbable
	1-3
	1-3
	4-6
	
	L
	Low Risk
	Proceed with task having implemented all identified controls

	
	
	Minor
	Moderate
	Serious Injury
	
	NOTE: Prior to the commencement of works any new Risk Assessments that have been prepared on site must be sent to the H&S Department for review and uploading on the shared drive.

	

	Photographs

	

	Key Points / Good Practice

	

	

	

	

	

	

	

	On each site and each location, the generic assessment below must be reviewed to ensure that all significant hazards and their risks are identified and controlled.  Please fill in the number of people who are directly affected.

This side of the Assessment must be filled in to make the Risk Assessment site specific.

	SITE / LOCATION: 
ACTIVITY:
Operating a Dumper
ADDITIONAL SPECIFIC HAZARDS:

ADDITIONAL CONTROL MEASURES:

ASSESSMENT OF REMAINING RISKS:   Low /Medium / High
	EMERGENCY PROCEDURES

ARE EMERGENCY PROCEDURES REQUIRED FOR THIS OPERATION: Yes  /  No

Name of competent person(s) appointed to take action.

TICK WHICH MAY REQUIRE ADDITIONAL ASSESSMENT TO BE DONE.

MANUAL

HANDLING

NOISE

COSHH

Method

Statement

OTHER

CIRCULATION OF RISK ASSESSMENT:

Tick Box

Contact and Emergency Numbers
Safety Department 

Site File
Brief operatives on assessments 
Revision

ON-SITE ASSESSMENT SIGNED:                                                        Date:

POSITION:


	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Operating a Dumper
	Ref: DGC_RA_0010

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Operating a Dumper
	Ref: DGC_RA_0010

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Operating a Dumper
	Ref: DGC_RA_0010

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:


Likelihood





Severity
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