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	HEALTH & SAFETY RISK ASSESSMENT

	Activity:
	Reducing Site Levels and Removal of Topsoil
	Site:
	
	Ref No:
	DGC_RA_0011

	Completed by:
	
	Position:
	Director
	Signed:
	
	Date:
	

	Who may be affected (Number of People?)

	Directly Affected:
	Employee
	4
	Subcontractors
	1
	Official visitors
	0
	General public
	0
	Indirectly Affected
	10

	Initial Risk
Before control measures are put in place
	Control Measures
	Residual Risk

After control measures are put in place

	No
	Hazards 
	L
	X
	S
	Score
	H/M/L
	Description
	L
	X
	S
	Score
	H/M/L

	1
	Pedestrians/Operatives colliding with site plant & vehicles
	3
	X
	3
	9
	H
	1. Pedestrians MUST be always segregated from mobile plant and vehicles on site.
2. Dedicated walkway and crossing point to be erected following Dandara site set up procedure.

3. Signage to be displayed informing site plant & vehicles of the speed limits and where pedestrians may be crossing.

4. All mobile plant must have a flashing orange beacon switched on when operating.

5. Signage to be displayed informing pedestrians of plant crossing points.

6. Pedestrians to give way to plant & vehicles on site, especially at crossing points.

7. An up-to-date traffic plan should be displayed on site for all to see and communicated to all operatives at induction and when there are changes to the plan.

8. Clearly marked routes for tipper. 
9. Arrangements for public safety re: - vehicles entering and leaving the site must be put into place in accordance with the New Road and Street Works Act and adequate ‘site entrance’ warnings displayed. 
10. All operatives involved with the work must be qualified and experienced and all machine drivers must have appropriate Competency cards.

11. Site traffic routes must be part of the site induction and updated on a regular basis; changes must be given to all site operatives via toolbox talks.
	1

	X
	1
	1
	L

	2
	Operation of Tipper Trucks
	3
	X
	3
	9
	H
	1. When excavated soil is to be removed from site by tipper trucks the wheel wash on site must be operational to clean the truck prior to leaving site preventing mud from contaminating the public highway.

2. A street sweeper is required to clean the roads when soil is being removed from site.
	1

	X
	1
	1
	L

	3
	Operation of site dumper
	3
	X
	3
	9
	H
	1. Dumper truck drivers are to apply handbrake, dismount from the dumper and stand in a safe location whilst the dumper is being loaded.

2. All dumper operators must be trained and competent to operate site dumper-NPORS/CPCS
3. All changes in levels as the work progresses must have safe inclines to ensure no risk of vehicles overturning.
4. Operators are to only use designated haul routes as laid out on the site traffic management plan.
5. Only use designated haul routes as laid out on the site traffic management plan.
	1

	X
	1
	1
	L

	4
	Loading of site dumper
	2
	X
	3
	6
	M
	1. Excavator operator to ensure that the dumper operator has dismounted and in a safe location before loading the dumper.

2. Excavator operator is not to push the dumper with the bucket of the excavator as this damages the handbrake of the dumper.

3. Excavator operator is not to overload the dumper.
	1

	X
	1
	1
	L

	5
	Striking Live Buried Services
	3
	X
	3
	9
	H
	1. Permit to dig/break ground required and all operatives to be briefed.

2. Banksman to attend all times during digging operations

3. Prior to excavating/reducing levels all existing service location drawings must be available and referred.

4. The area to be excavated/reduced must be scanned using a cable avoidance tool and the ground marked where it has located a service. No mechanical digging or the use of power tools within 500mm of any buried services, Treat All Buried Services as Live

5. Safe hand digging practices must be adopted to confirm the location of the service and the direction it is running in. 

6. All underground services must be marked on site before any work commences.  CAT Scan & locate.
7. Only use insulated tools when carrying out hand digs.

8. Operatives to wear ARC rated PPE during any excavation work in/near live services.
	2
	X
	1
	2
	L

	6
	Security
	3
	X
	3
	9
	H
	1. Ensure that the area being excavated/reduced is secure only permitting access to authorised personnel. 

2. Adequate temporary fencing & signage must be put into place around the full site boundary. 2m high site boundary fencing must be erected as soon as practically possible.
	1
	X
	1
	1
	L

	7
	Hazardous fill material
	2
	X
	2
	4
	M
	1. The fill must be examined as the work progresses to ensure correct safe handling and disposal. 

2. The ground being excavated must be continuously checked for any signs of contamination as the work progresses.  Work must stop if any material/substance or liquid is found other than sand/soil/clay or groundwater.
	1
	X
	1
	1
	L

	8
	Collapse of Excavation 
	3
	X
	3
	9
	H
	1. Appropriate checks must be made to ensure no underground voids exist. 

2. The angle of repose of excavated materials topsoil stored on site must be a maximum of 30%.
3. Excavation inspection register is to be maintained throughout excavation works.
	1
	X
	1
	1
	L

	
	
	
	
	
	
	
	Refer to Toolbox Talks CITB_C08, CITB_C09, CITB_C21, CITB_D11, CITB_E1, CITB_9.9_03, HS_9.9_06, HS_9.9_10, HS_9.9_11, HS_9.9_48, HS_9.9_52
	
	
	
	
	

	
	
	
	
	
	
	
	MANDATORY PPE – Hard hat, High-viz vest, Safety boots with steel toe and mid-sole 
	
	
	
	
	

	
	
	
	
	
	
	
	ADDITIONAL PPE REQUIRED – 
	
	
	
	
	

	Likelihood (L)
	Severity (S)
	Score (Likelihood x Severity) (LXS)
	Rating

	1 = Improbable
	1 = Minor
	7 - 9
	High

	2 = Probable
	2 = Moderate
	4 – 6
	Medium

	3 = Certain
	3 = Serious Injury
	1 - 3
	Low
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	Certain
	4-6
	7-9
	7-9
	
	H
	High Risk
	Additional control measures required to reduce the residual risk to an acceptable level. A full method statement must be provided with this risk assessment. Both must be communicated to all persons involved with the task prior to the commencement of the task.

	
	Probable
	1-3
	4-6
	7-9
	
	M
	Medium Risk
	Ensure that identified control measures are adequate. Are there further control measures which could be implemented to lower the risk?

	
	Improbable
	1-3
	1-3
	4-6
	
	L
	Low Risk
	Proceed with task having implemented all identified controls

	
	
	Minor
	Moderate
	Serious Injury
	
	NOTE: Prior to the commencement of works any new Risk Assessments that have been prepared on site must be sent to the H&S Department for review and uploading on the shared drive.

	

	Photographs


	

	Key Points / Good Practice

	

	

	

	

	

	

	

	On each site and each location, the generic assessment below must be reviewed to ensure that all significant hazards and their risks are identified and controlled.  Please fill in the number of people who are directly affected.

This side of the Assessment must be filled in to make the Risk Assessment site specific.

	SITE / LOCATION: 
ACTIVITY:

Reducing Site Levels and Removal of Topsoil
ADDITIONAL SPECIFIC HAZARDS:

ADDITIONAL CONTROL MEASURES:

ASSESSMENT OF REMAINING RISKS:   Low /Medium / High
	EMERGENCY PROCEDURES

ARE EMERGENCY PROCEDURES REQUIRED FOR THIS OPERATION: Yes  /  No

Name of competent person(s) appointed to take action.

TICK WHICH MAY REQUIRE ADDITIONAL ASSESSMENT TO BE DONE.

MANUAL

HANDLING

NOISE

COSHH

Method

Statement

OTHER

CIRCULATION OF RISK ASSESSMENT:

Tick Box

Contact and Emergency Numbers
Safety Department 

Site File
Brief operatives on assessments 
Revision

ON-SITE ASSESSMENT SIGNED:                                                        Date:

POSITION:


	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Reducing Site Levels and Removal of Topsoil
	Ref: DGC_RA_0011

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Reducing Site Levels and Removal of Topsoil
	Ref: DGC_RA_0011

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Reducing Site Levels and Removal of Topsoil
	Ref: DGC_RA_0011

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:


Likelihood





Severity
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