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	HEALTH & SAFETY RISK ASSESSMENT 

	Activity:
	Working with Live Manholes & Sewage Systems 
	Site:
	
	Ref No:
	DGC_RA_0019

	Completed by:
	
	Position:
	Director
	Signed:
	
	Date:
	

	Who may be affected (Number of People?)

	Directly Affected:
	Employee
	5
	Subcontractors
	1
	Official visitors
	0
	General public
	5+
	Indirectly Affected
	12

	Initial Risk
Before control measures are put in place
	Control Measures
	Residual Risk

After control measures are put in place

	No
	Hazards 
	L
	X
	S
	Score
	H/M/L
	Description
	L
	X
	S
	Score
	H/M/L

	1
	Limb/back and foot\hand injuries
	3
	X
	3
	9
	H
	Where lifting involved a manual handling risk assessment to be completed and all operatives are manual handling trained, see Dandara safety procedure DA-HSP-32 Manual Handling.
Ensure correct tools are used – suitable manhole keys, mechanical lifter (if possible), block and roller for heavy covers. 

Ensure covers are free before attempting to lift.
	1
	X
	1
	1
	L

	2
	Contact with foul water/sewage = Infection, illness from ingested water etc.
	3
	X
	3
	9
	H
	RAMS required for emergency rescue along with a permit to enter these are to be issued daily and all operatives trained in recovery rescue. All operative to be inducted daily in their operations and must sign to say they have received them and understood them.

If breathing apparatus required then all personnel must be trained in their use, copies of training must be attached to their site induction sheets.
COSHH assessment required, and all operatives inducted in its contents.
Wear protective footwear and heavy-duty gloves. 

Ensure personal protective equipment is worn – rubber gloves, disposable or waterproof coveralls, Wellington boots (steel toe & mid-sole), eye and/or face protection, respirator etc. 

Treat cuts immediately by cleaning and using a waterproof plaster.

Where necessary showers may have to be provided. 
	2
	X
	1
	2
	L

	3
	Rodding of drains to clear blockages
	2
	X
	2
	4
	M
	Clean/disinfect equipment after use. 


	1
	X
	1
	1
	L

	4
	Lifting manhole covers, Presence of flammable or asphyxiating gases
	3
	X
	3
	9
	H
	Only operatives with confined space training are allowed to enter confined spaces. 

All confined space equipment must be available, e.g. Tripod, winch, safety harness etc in manholes.
Operatives given training in awareness of residual gas builds up and the procedures for dealing with it, i.e. by venting away flammable or asphyxiating gases. No smoking, no naked lights and warning signs to be displayed. If gas testing equipment is to be used operatives to be trained in its use.
	1
	X
	1
	1
	L

	5
	Use of drain cleaning fluids etc. Skin contact with chemical cleaners etc.
	3
	X
	3
	9
	H
	Ensure good personal hygiene, washing with hot water (particularly before eating or drinking). 

COSHH assessments to be carried out prior to use. Manufacturer’s instructions to be always followed for use, storage and disposal. Appropriate PPE to be worn.
	2
	X
	1
	2
	L

	
	
	
	
	
	
	
	Refer to Toolbox Talks CIRIA_05, CITB_B03, CITB_B07, CITB_B09, CITB_B17, CITB_B19, CITB_D08, CITB_D12, HS_9.9_37, HS_9.9_48, HS_9.9_53
	
	
	
	
	

	
	
	
	
	
	
	
	MANDATORY PPE – Hard hat, High-viz vest, Safety boots with steel toe and mid-sole 
	
	
	
	
	

	
	
	
	
	
	
	
	ADDITIONAL PPE REQUIRED – FFP3 mask, Keep safe PVC gauntlet gloves, Gas monitor, Full body harness, Tripod
	
	
	
	
	

	Likelihood (L)
	Severity (S)
	Score (Likelihood x Severity) (LXS)
	Rating

	1 = Improbable
	1 = Minor
	7 - 9
	High

	2 = Probable
	2 = Moderate
	4 – 6
	Medium

	3 = Certain
	3 = Serious Injury
	1 - 3
	Low
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	Certain
	4-6
	7-9
	7-9
	
	H
	High Risk
	Additional control measures required to reduce the residual risk to an acceptable level. A full method statement must be provided with this risk assessment. Both must be communicated to all persons involved with the task prior to the commencement of the task.

	
	Probable
	1-3
	4-6
	7-9
	
	M
	Medium Risk
	Ensure that identified control measures are adequate. Are there further control measures which could be implemented to lower the risk?

	
	Improbable
	1-3
	1-3
	4-6
	
	L
	Low Risk
	Proceed with task having implemented all identified controls

	
	
	Minor
	Moderate
	Serious Injury
	
	NOTE: Prior to the commencement of works any new Risk Assessments that have been prepared on site must be sent to the H&S Department for review and uploading on the shared drive.

	

	Photographs


	

	Key Points / Good Practice



	

	

	

	

	

	

	

	

	

	

	

	

	

	On each site and each location, the generic assessment below must be reviewed to ensure that all significant hazards and their risks are identified and controlled.  Please fill in the number of people who are directly affected.

This side of the Assessment must be filled in to make the Risk Assessment site specific.

	SITE / LOCATION: 
ACTIVITY:

Working with Live Manholes & Sewage Systems
ADDITIONAL SPECIFIC HAZARDS:

ADDITIONAL CONTROL MEASURES:

ASSESSMENT OF REMAINING RISKS:   Low /Medium / High
	EMERGENCY PROCEDURES

ARE EMERGENCY PROCEDURES REQUIRED FOR THIS OPERATION: Yes  /  No

Name of competent person(s) appointed to take action.

TICK WHICH MAY REQUIRE ADDITIONAL ASSESSMENT TO BE DONE.

MANUAL

HANDLING

NOISE

COSHH

Method

Statement

OTHER

CIRCULATION OF RISK ASSESSMENT:

Tick Box

Contact and Emergency Numbers
Safety Department 

Site File
Brief operatives on assessments 
Revision

ON-SITE ASSESSMENT SIGNED:                                                        Date:

POSITION:


	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Working with Live Manholes & Sewage Systems
	Ref: DGC_RA_0019

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Working with Live Manholes & Sewage Systems
	Ref: DGC_RA_0019

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Working with Live Manholes & Sewage Systems
	Ref: DGC_RA_0019

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:


Likelihood





Severity
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