
[image: image4]

	HEALTH & SAFETY RISK ASSESSMENT

	Activity:
	Road Construction – Kerb Base 
	Site:
	
	Ref No:
	DA_RA_0023

	Completed by:
	
	Position:
	Director
	Signed:
	
	Date:
	

	Who may be affected (Number of People?)

	Directly Affected:
	Employee
	6
	Subcontractors
	1
	Official visitors
	0
	General public
	0
	Indirectly Affected
	10

	Initial Risk
Before control measures are put in place
	Control Measures
	Residual Risk

After control measures are put in place

	No
	Hazards 
	L
	X
	S
	Score
	H/M/L
	Description
	L
	X
	S
	Score
	H/M/L

	1
	Moving plant
	3
	X
	3
	9
	H
	1. If works are in the public highway, then secure barriers & signage to be in place.  Safety in Street Works & Road Works a Code of Practice enforced, 

2. Flashing beacons to be used if works are in place during poor visibility or at night. Contact numbers to be displayed

3. Banksmen must always be used. All Plant Operators must be made aware of pedestrian routes to reduce the risk of plant & pedestrian conflict.

4. All works on the public highways to be inspected each morning and at the end of the working day as a minimum by site management this to be recorded

5. Safety department to inspect on a daily basis again this to be recorded
	1
	X
	1
	1
	L

	2
	Slips, trips & falls
Contact with loose debris / stones. 

Ankle injuries


	3
	X
	3
	9
	H
	All manholes must have covers fixed into place. If temporary covers are used, they must be of a suitable thickness & be fixed into position to prevent movement & marked void below. 

Ensure all pedestrian routes are kept clear and free from any obstructions, any steps are sanded or ramped. This must be inspected regularly throughout the day especially where members of the public are involved, these inspections must be recorded 

Crowd barriers must be erected for safety of pedestrians & vehicles for works open for short durations, however, for works open for long periods Heras fencing must be erected.
Ongoing housekeeping to be applied by all operatives and monitored by Site Supervisor. 
Work in coordination with the Telehandler Operator to set up a safe area for plant, materials and waste skip. 
As needed use a combination of site plant with fit for purpose attachments and manual brush sweeping to keep work area free from loose stone, rubble and debris. 

	2
	X
	1
	2
	L

	4
	Use of a Stihl saw
	3
	X
	3
	9
	H
	Stihl saw only to be used by trained and competent operator.

Dust suppression/Extraction to be always used
Only trained abrasive wheel operators are allowed to change the discs 

All PPE must be always worn when operating the saw i.e. FFP3 dust masks, impact goggles, ear defenders, hi vis, safety boots, safety gloves and hard hat
HAV management and exposure logs must be always completed during any operation of this equipment.


	1
	X
	1
	1
	L

	5
	Manual handling
	3
	X
	3
	9
	H
	Where possible/practicable mechanical lifting is to be used, should this not be possible, a manual handling risk assessment must be completed, and all operatives trained in manual handling.

Wheelbarrow safety.
Do not overfill the wheelbarrow.
 Make sure that the wheelbarrow’s tyres are pumped up. 

When lifting the wheelbarrow, make sure that you bend your knees and lift with your legs, not your back.
Do not try to climb or descend inclines that are too steep for you.
	2
	X
	1
	2
	L

	6
	Dust
	3
	X
	3
	9
	H
	If Stihl saw is to be used to cut blocks, dust suppression/M rated extraction must be always used, see item 3 for the PPE/RPE to be worn.
If dry cutting of kerbs takes place it must be undertaken in a well-ventilated area and dust suppression/extraction MUST be used, with Operatives being ’face fit tested’ for FFP3 dust mask & dust mask MUST worn.

	2
	X
	1
	2
	L

	7
	Cement/Concrete
	3
	X
	3
	9
	H
	COSHH assessment must be completed, and all operatives must be inducted in this. Operatives must sign the COSHH assessment

PPE to worn as per the COSHH assessment, which should state, eye protection, skin protection
	1
	X
	1
	1
	L

	8
	Noise
	3
	X
	3
	9
	H
	Ear Defenders must be worn for cutting operations.
	1
	X
	1
	1
	L

	9
	Underground Services
	3
	X
	3
	9
	H
	Permit to dig/break ground must be completed before trying to locate underground services. No Permit No Dig

No plant or power tools to be operated within 500mm of any underground service. Treat all services as live

Hand Dig only to locate services, no mechanical digging within 500mm of a known buried service.
Banksman, to attend all times
Insulated tools to be always used.

ARC rated PPE must be worn by operatives exposing or potentially working on/near any known live services.
	1
	X
	1
	1
	L

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Refer to Toolbox Talks CITB_B11, CITB_B19, CITB_C08, CITB_D11, CITB_F02, HS_9.9_03, HS_9.9_27, HS_9.9_48, HS_9.9_52.
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	MANDATORY PPE – Hard hat, High-viz vest, Safety boots with steel toe and mid-sole 
	
	
	
	
	

	
	
	
	
	
	
	
	ADDITIONAL PPE REQUIRED – Safety goggles, FFP3 mask, Level 1 gloves, Ear defenders
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	
	

	Likelihood (L)
	Severity (S)
	Score (Likelihood x Severity) (LXS)
	Rating

	1 = Improbable
	1 = Minor
	7 - 9
	High

	2 = Probable
	2 = Moderate
	4 – 6
	Medium

	3 = Certain
	3 = Serious Injury
	1 - 3
	Low
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	Certain
	4-6
	7-9
	7-9
	
	H
	High Risk
	Additional control measures required to reduce the residual risk to an acceptable level. A full method statement must be provided with this risk assessment. Both must be communicated to all persons involved with the task prior to the commencement of the task.

	
	Probable
	1-3
	4-6
	7-9
	
	M
	Medium Risk
	Ensure that identified control measures are adequate. Are there further control measures which could be implemented to lower the risk?

	
	Improbable
	1-3
	1-3
	4-6
	
	L
	Low Risk
	Proceed with task having implemented all identified controls

	
	
	Minor
	Moderate
	Serious Injury
	
	NOTE: Prior to the commencement of works any new Risk Assessments that have been prepared on site must be sent to the H&S Department for review and uploading on the shared drive.

	

	Photographs
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	Ensure clear signage in place & visible to oncoming vehicles
	Ensure clear signage in place & visible to oncoming vehicles
	Sand or ramp any deviations in pavement levels

	Key Points / Good Practice

	Site personnel inducted
	Toolbox talk given on water dust suppression when cutting with Stihl saw

	Plant Operators to be competent & hold a current competency card
	Toolbox talk given on hazards associated with Cement/Concrete

	Only competent personnel to change abrasive wheels
	Area of dig to be CAT scanned

	Daily street works inspections for works in public highway
	Utilities companies contacted; services marked & identified

	COSHH assessment in place for Cement/Concrete
	Site services drawing available

	Emergency eye was station available
	Permit to dig in place

	Manholes covered & identified
	Face fit testing for dust masks

	Pertinent site signage in place
	

	
	

	
	

	
	

	On each site and each location, the generic assessment below must be reviewed to ensure that all significant hazards and their risks are identified and controlled.  Please fill in the number of people who are directly affected.

This side of the Assessment must be filled in to make the Risk Assessment site specific.

	SITE / LOCATION: 
ACTIVITY:

Road Construction – Kerb Base
ADDITIONAL SPECIFIC HAZARDS:

ADDITIONAL CONTROL MEASURES:

ASSESSMENT OF REMAINING RISKS:   Low /Medium / High
	EMERGENCY PROCEDURES

ARE EMERGENCY PROCEDURES REQUIRED FOR THIS OPERATION: Yes / No
Name of competent person(s) appointed to take action.

TICK WHICH MAY REQUIRE ADDITIONAL ASSESSMENT TO BE DONE.

MANUAL

HANDLING

NOISE

COSHH

Method

Statement

OTHER

CIRCULATION OF RISK ASSESSMENT:

Tick Box

Contact and Emergency Numbers
Safety Department 

Site File

Brief operatives on assessments 
Revision

ON-SITE ASSESSMENT SIGNED:                                                        Date:

POSITION:


	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Road Construction – Kerb Base
	Ref: DGC_RA_0023

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Road Construction – Kerb Base
	Ref: DGC_RA_0023

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Road Construction – Kerb Base
	Ref: DGC_RA_0023

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:


Likelihood





Severity








DGC_RA_0023 Road Construction Kerb Base                                                                                                                                                                                April 2026

