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	HEALTH & SAFETY RISK ASSESSMENT 

	Activity:
	Working with Rebar and Steel Mesh
	Site:
	
	Ref No:
	ICP_RA_0024

	Completed by:
	
	Position:
	Director
	Signed:
	
	Date:
	

	Who may be affected (Number of People?)

	Directly Affected:
	Employee
	4
	Subcontractors
	1
	Official visitors
	0
	General public
	0
	Indirectly Affected
	8

	Initial Risk
Before control measures are put in place
	Control Measures
	Residual Risk

After control measures are put in place

	No
	Hazards 
	L
	X
	S
	Score
	H/M/L
	Description
	L
	X
	S
	Score
	H/M/L

	1
	Cuts / Abrasions / Puncture Wounds
	3
	X
	3
	9
	H
	1. Be aware of sharp edges on rebar and steel mesh ends and possibility of whipping effect of mesh and coils of steel wire particularly when wire and mesh is being cut.

2. Safety gloves to be always worn when handling or working with rebar and steel mesh, particularly when tying mesh & rebar together or wire is being cut. 

3. When tying rebar and mesh ensure that the wire is twisted tight prior to cutting and that the twisted tail of the wire is turned back into the joint to prevent cuts and snags. Ensure the tail does not encroach into the external face of the concrete covering.
	2
	X
	1
	2
	L

	2
	Manual Handling
	3
	X
	3
	9
	H
	1. Packs of Steel Mesh and Rebar to be mechanically lifted into place prior to decanting to final positioning.

2. Use of mechanical handling equipment where possible, if this is not possible then a manual handling risk assessment is required, and all operatives trained in manual handling. See Dandara safety procedure DA-HSP-32 Manual Handling.
3. Large pieces of mesh or tied rebar cages to be mechanically lifted into position e.g. when lowering mesh into retaining walls etc.  
	1
	X
	1
	1
	L

	3
	Flying Particles (eye injuries)
	3
	X
	3
	9
	H
	1. Safety glasses or impact resistant goggles to be worn where there is a possibility of whipping effect from mesh or coils of wire or flying particles when wire is cut.

2. Wear safety goggles, safety gloves and ear defenders when cutting rebar and mesh with abrasive disc cutters (Stihl saws)
	2
	X
	1
	2
	L

	4
	Slips, Trips & Falls
	3
	X
	3
	9
	H
	1. If there is a need to walk across previously laid steel mesh or rebar, ensure that the route taken is secure and stable, and be mindful of potential tripping hazards e.g. gaps in mesh. 

2. Off cuts of mesh and rebar to be disposed of in the waste metal skip and not left lying around on-site causing tripping hazards. This is to be carried out on a regular basis throughout the working day

3. Mushroom caps must be fitted to both vertical and horizontal ends of rebar and mesh to prevent injury. 
	1
	X
	1
	1
	L

	5
	Working at Height
	2
	X
	2
	4
	M
	1. When working at height, suitable fall protection to be put in place e.g. external scaffold platform & Guard rails, these must be suitably tied or braced. 

2. Openings in raised floor slab installations e.g. stair wells, service risers to have suitable fall protection e.g. guard rails, covers.

3. Work areas to be cordoned off above and below works to prevent unauthorised access.
	1
	X
	1
	1
	L

	6
	Moving Plant
	3
	X
	3
	9
	H
	Work area to be segregated from any moving plant.   
	1
	X
	1
	1
	L

	7
	Noise 
	2
	X
	2
	4
	M
	Wear safety goggles, safety gloves and ear defenders when cutting rebar and mesh with abrasive disc cutters (Stihl saws)
	1
	X
	1
	1
	L

	8
	Fire 
	2
	X
	2
	4
	M
	1. Hot works permit required, and this is to be issued daily. Fire watch is required 60 mins before shift ends

2. When cutting rebar and mesh with abrasive disc cutters (Stihl saws), ensure that the mesh or rebar is secure and will not move, that any Sparks created are not directed where there is a possibility to cause fire or damage to surroundings, that they are not directed into walkways or where other operatives are working.

3. Ensure that a fire extinguisher is easily to hand when cutting rebar and mesh with abrasive wheels (Stihl saws) and when refuelling petrol driven abrasive wheels.
	1
	X
	1
	1
	L

	
	
	
	
	
	
	
	MANDATORY PPE – Hard hat, High-viz vest, Safety boots with steel toe and mid-sole 
	
	
	
	
	

	
	
	
	
	
	
	
	ADDITIONAL PPE REQUIRED – 
	
	
	
	
	

	Likelihood (L)
	Severity (S)
	Score (Likelihood x Severity) (LXS)
	Rating

	1 = Improbable
	1 = Minor
	7 - 9
	High

	2 = Probable
	2 = Moderate
	4 – 6
	Medium

	3 = Certain
	3 = Serious Injury
	1 - 3
	Low
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	Certain
	4-6
	7-9
	7-9
	
	H
	High Risk
	Additional control measures required to reduce the residual risk to an acceptable level. A full method statement must be provided with this risk assessment. Both must be communicated to all persons involved with the task prior to the commencement of the task.

	
	Probable
	1-3
	4-6
	7-9
	
	M
	Medium Risk
	Ensure that identified control measures are adequate. Are there further control measures which could be implemented to lower the risk?

	
	Improbable
	1-3
	1-3
	4-6
	
	L
	Low Risk
	Proceed with task having implemented all identified controls

	
	
	Minor
	Moderate
	Serious Injury
	
	NOTE: Prior to the commencement of works any new Risk Assessments that have been prepared on site must be sent to the H&S Department for review and uploading on the shared drive.

	

	Photographs

	

	Key Points / Good Practice

	

	

	

	

	

	

	

	On each site and each location, the generic assessment below must be reviewed to ensure that all significant hazards and their risks are identified and controlled.  Please fill in the number of people who are directly affected.

This side of the Assessment must be filled in to make the Risk Assessment site specific.

	SITE / LOCATION: 
ACTIVITY:

Working with Rebar and Steel Mesh
ADDITIONAL SPECIFIC HAZARDS:

ADDITIONAL CONTROL MEASURES:

ASSESSMENT OF REMAINING RISKS:   Low /Medium / High


	EMERGENCY PROCEDURES

ARE EMERGENCY PROCEDURES REQUIRED FOR THIS OPERATION: Yes  /  No

Name of competent person(s) appointed to take action.

TICK WHICH MAY REQUIRE ADDITIONAL ASSESSMENT TO BE DONE.

MANUAL

HANDLING

NOISE

COSHH

Method

Statement

OTHER

CIRCULATION OF RISK ASSESSMENT:

Tick Box

Contact and Emergency Numbers
Safety Department 

Site File

Brief operatives on assessments 
Revision

ON-SITE ASSESSMENT SIGNED:                                                        Date:

POSITION:


	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Working with Rebar and Steel Mesh
	Ref: DGC_RA_0024

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Working with Rebar and Steel Mesh
	Ref: DGC_RA_0024

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Working with Rebar and Steel Mesh
	Ref: DGC_RA_0024

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:


Likelihood





Severity
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