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	HEALTH & SAFETY RISK ASSESSMENT 

	Activity:
	Vehicle Marshalling 
	Site:
	
	Ref No:
	DGC_RA_0025

	Completed by:
	
	Position:
	Director
	Signed:
	
	Date:
	

	Who may be affected (Number of People?)

	Directly Affected:
	Employee
	2
	Subcontractors
	2
	Official visitors
	2
	General public
	10+
	Indirectly Affected
	20+

	Initial Risk
Before control measures are put in place
	Control Measures
	Residual Risk

After control measures are put in place

	No
	Hazards 
	L
	X
	S
	Score
	H/M/L
	Description
	L
	X
	S
	Score
	H/M/L

	1
	Struck by moving vehicles
	3
	x
	3
	9
	H
	1. All vehicle marshals must be trained and competent to marshal any vehicles (copy of proof of training to be retained by site management)
2. No marshalling of any vehicles is to be carried out by anyone who is not qualified as a vehicle marshal.

3. All vehicle marshals are to wear a Half Yellow/Half Orange Hi Viz Vest with “Vehicle Marshal” written on the back whilst vehicle marshalling.

4. Where a vehicle marshal is required on public roads, two vehicle marshals will be required.
5. Follow the highway code

6. Prior to carrying out any manoeuvres the vehicle marshal and vehicle driver must discuss what is to happen. 

7. Vehicle marshals are to ensure that they remain visible to the driver of the vehicle they are marshalling.

8. Be mindful that European lorries are driven from the left-hand side unlike the UK where they are right hand drive 

9. Where necessary 2 or more vehicle marshals may be required to carry out the manoeuver.

10. If direct line of site is blocked or if you are unsure, stop the manoeuver and reposition yourself to a better viewpoint.
11. If required, barrier off area to keep unauthorised persons walking into the manoeuvring area.
	1
	x
	1
	1
	L

	2
	Vehicle colliding with stationary objects
	3
	x
	3
	9
	H
	1. The vehicle marshal must always use the correct signalling when marshalling a vehicle.
2. Mobile phones are not to be used when manoeuvers are being carried out.

3. Be aware of scaffolding and overhangs from buildings. Be mindful of overhead services
4. If marshalling a vehicle into a building, check the height of the vehicle and opening prior to carrying out the manoeuver.
	2
	x
	1
	2
	L

	3
	Vehicle falling into excavation / excavation collapse
	3
	x
	3
	9
	H
	1. Where possible, stop blocks are to be positioned a minimum of 4m from an excavation to prevent the vehicle falling in and to prevent any excess load to the walls which may cause the excavation to collapse.
	2
	x
	1
	2
	L

	4
	Crush Injury
	3
	x
	3
	9
	H
	1. Vehicle Marshals are to stay clear of the tailgate of tipper trucks when tipping, watch out for the swing of the tailgate.
	1
	x
	1
	1
	L

	5
	Injury to the Public
	3
	x
	3
	9
	H
	1. Vehicle Marshals must be aware of the pedestrians in the area when manoeuvring. If safe to do so, stop the manoeuver and allow the pedestrian(s) to pass.

2. Always be aware of public vehicle movements 
	2
	x
	1
	2
	L

	6
	General
	2
	x
	2
	4
	M
	1. Where possible arrange for works or deliveries to occur at quieter periods during the day avoiding morning and evening rush hours.

2. Delivery drivers to be site inducted and made aware of signal procedures prior to entering site
	1
	x
	1
	1
	L

	
	
	
	
	
	
	
	MANDATORY PPE – Hard hat, Half Yellow/Half Orange High-viz vest with Vehicle Marshal written on the back, Safety boots with steel toe and mid-sole 
	
	
	
	
	

	
	
	
	
	
	
	
	ADDITIONAL PPE REQUIRED – 
	
	
	
	
	

	Likelihood (L)
	Severity (S)
	Score (Likelihood x Severity) (LXS)
	Rating

	1 = Improbable
	1 = Minor
	7 - 9
	High

	2 = Probable
	2 = Moderate
	4 – 6
	Medium

	3 = Certain
	3 = Serious Injury
	1 - 3
	Low

	[image: image1][image: image2.png]START
Attention
Start of
Command

STOP
Interruption
End of
movement

of the
operation

both arms are extended
horizontally with the palms
facing forwards.

the right arm points upwards
with the palm facing forwards.

both hands are clasped at
chest height.





	Certain
	4-6
	7-9
	7-9
	
	H
	High Risk
	Additional control measures required to reduce the residual risk to an acceptable level. A full method statement must be provided with this risk assessment. Both must be communicated to all persons involved with the task prior to the commencement of the task.

	
	Probable
	1-3
	4-6
	7-9
	
	M
	Medium Risk
	Ensure that identified control measures are adequate. Are there further control measures which could be implemented to lower the risk?

	
	Improbable
	1-3
	1-3
	4-6
	
	L
	Low Risk
	Proceed with task having implemented all identified controls

	
	
	Minor
	Moderate
	Serious Injury
	
	NOTE: Prior to the commencement of works any new Risk Assessments that have been prepared on site must be sent to the H&S Department for review and uploading on the shared drive.
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	Photographs
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	Key Points / Good Practice

	

	

	

	

	On each site and each location, the generic assessment below must be reviewed to ensure that all significant hazards and their risks are identified and controlled.  Please fill in the number of people who are directly affected.

This side of the Assessment must be filled in to make the Risk Assessment site specific.

	SITE / LOCATION: 
ACTIVITY:

Vehicle Marshalling 
ADDITIONAL SPECIFIC HAZARDS:

ADDITIONAL CONTROL MEASURES:

ASSESSMENT OF REMAINING RISKS:   Low /Medium / High
	EMERGENCY PROCEDURES

ARE EMERGENCY PROCEDURES REQUIRED FOR THIS OPERATION: Yes  /  No

Name of competent person(s) appointed to take action.

TICK WHICH MAY REQUIRE ADDITIONAL ASSESSMENT TO BE DONE.

MANUAL

HANDLING

NOISE

COSHH

Method

Statement

OTHER

CIRCULATION OF RISK ASSESSMENT:

Tick Box

Contact and Emergency Numbers
Safety Department 

Site File
Brief operatives on assessments 
Revision

ON-SITE ASSESSMENT SIGNED:                                                        Date:

POSITION:


	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Vehicle Marshalling 
	Ref: DGC_RA_0025
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	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Vehicle Marshalling 
	Ref: DGC_RA_0025

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Vehicle Marshalling 
	Ref: DGC_RA_0025

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:


Likelihood





Severity








DGC_RA_0025 Vehicle Marshalling                                                                                                                                                                                                      April 2026

