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	HEALTH & SAFETY RISK ASSESSMENT

	Activity:
	Laying of Block Paviours 
	Site:
	
	Ref No:
	DGC_RA_0027

	Completed by:
	
	Position:
	Director
	Signed:
	
	Date:
	

	Who may be affected (Number of People?)

	Directly Affected:
	Employee
	3
	Subcontractors
	1
	Official visitors
	0
	General public
	10+
	Indirectly Affected
	20

	Initial Risk
Before control measures are put in place
	Control Measures
	Residual Risk

After control measures are put in place

	No
	Hazards 
	L
	X
	S
	Score
	H/M/L
	Description
	L
	X
	S
	Score
	H/M/L

	1
	Slips, trips & falls
	3
	X
	3
	9
	H
	1. All open roadside gullies, manholes, telecom boxes etc. to be covered to prevent falls. 

2. Any areas where laying of paviours cannot be completed e.g. up to a kerb edge or road gulley then steps & gaps to be covered to eliminate tripping hazards. 

3. Ensure that the area being worked is kept tidy with materials kept in an orderly fashion & waste e.g. block off-cuts cleared at regular intervals during & at the end of shift.
	1
	X
	1
	1
	L

	2
	Noise
	3
	X
	3
	9
	H
	When levelling sand or block using a Wacker plate ear defenders are to be worn, this applies to Operators working in the radius of the activity.
	1
	X
	1
	1
	L

	3
	Dust
	3
	X
	3
	9
	H
	1. If blocks are to be cut using an abrasive wheel e.g. Stihl saw then ear defenders, safety goggles and FFP3 dust masks to be worn.  This applies to Operators working in a 2m radius of the activity – To be read in conjunction with DA_RA_0148 Using a Stihl Saw safe system of work.

2. Water suppression/M rated Dust extraction systems must be attached to the Stihl saw at all times. 

3. All operatives must always wear a FFP3 dust mask and operatives must have the dust mask face fit tested (FFT) 
	2
	X
	1
	2
	L

	4
	Flying debris
	3
	X
	3
	9
	H
	Use the correct tool for the job e.g. designed & fit for purpose. Impact goggles to be always worn. 
	1
	X
	1
	1
	L

	5
	Manual handling
	3
	X
	3
	9
	H
	1. Where practicable use mechanical handling devices (barrows, pallet trucks, forklifts) to move blocks, materials & equipment to loading out areas. 
2. Ensure Operators have received a manual handling toolbox talk and there is a Manual Handling Risk Assessment in place if Manual Handling cannot be avoided.
	1
	X
	1
	1
	L

	6
	Access
	2
	X
	3
	6
	M
	Board out of area adjacent to works to maintain access where necessary, whilst ensuring no slip or tripping hazards present, particularly where public access is required. 
	1
	X
	1
	1
	L

	7
	Hazardous substances
	2
	X
	2
	4
	M
	Read COSHH assessments of all products you will be using before use e.g. Cement.
	1
	X
	1
	1
	L

	8
	Moving Plant
	3
	X
	3
	9
	H
	If the base layer of sand is to be mechanically graded using a mini digger, digger driver to be suitably competent to drive machine (CPCS or Employers Federation card).
Adequate plant segregation must always be in place.
	2
	X
	1
	2
	L

	9
	Members of the Public
	3
	X
	3
	9
	H
	If working adjacent to the public highway e.g. pavement or road then works to be suitable barriered & signed to highway users.
M Rated dust extraction must be in place to protect members of the public and their property
	2
	X
	1
	2
	L

	10
	Vibration
	3
	X
	3
	9
	H
	Exposure logs are to be kept for all operatives using both the Stihl saw and or whacker plate as pat of the HAV management process and Dandara company policy.
	1
	X
	1
	1
	L

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	Refer to Toolbox Talks CITB_B15, CITB_B19, CITB_C07, CITB_C09, CITB_C10, HS_9.9_16, HS_9.9_52.
	
	
	
	
	

	
	
	
	
	
	
	
	MANDATORY PPE – Hard hat, High-viz vest, Safety boots with steel toe and mid-sole 
	
	
	
	
	

	
	
	
	
	
	
	
	ADDITIONAL PPE REQUIRED – Safety impact goggles, FFP3 mask, Level 1 gloves, Knee pads, Ear defenders  
	
	
	
	
	

	Likelihood (L)
	Severity (S)
	Score (Likelihood x Severity) (LXS)
	Rating

	1 = Improbable
	1 = Minor
	7 - 9
	High

	2 = Probable
	2 = Moderate
	4 – 6
	Medium

	3 = Certain
	3 = Serious Injury
	1 - 3
	Low
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	Certain
	4-6
	7-9
	7-9
	
	H
	High Risk
	Additional control measures required to reduce the residual risk to an acceptable level. A full method statement must be provided with this risk assessment. Both must be communicated to all persons involved with the task prior to the commencement of the task.

	
	Probable
	1-3
	4-6
	7-9
	
	M
	Medium Risk
	Ensure that identified control measures are adequate. Are there further control measures which could be implemented to lower the risk?

	
	Improbable
	1-3
	1-3
	4-6
	
	L
	Low Risk
	Proceed with task having implemented all identified controls

	
	
	Minor
	Moderate
	Serious Injury
	
	NOTE: Prior to the commencement of works any new Risk Assessments that have been prepared on site must be sent to the H&S Department for review and uploading on the shared drive.

	

	Photographs

	

	Key Points / Good Practice

	

	

	

	

	

	

	

	

	

	On each site and each location, the generic assessment below must be reviewed to ensure that all significant hazards and their risks are identified and controlled.  Please fill in the number of people who are directly affected.

This side of the Assessment must be filled in to make the Risk Assessment site specific.

	SITE / LOCATION: 
ACTIVITY:

Laying of Block Paviors
ADDITIONAL SPECIFIC HAZARDS:

ADDITIONAL CONTROL MEASURES:

ASSESSMENT OF REMAINING RISKS:   Low /Medium / High
	EMERGENCY PROCEDURES

ARE EMERGENCY PROCEDURES REQUIRED FOR THIS OPERATION: Yes  /  No

Name of competent person(s) appointed to take action.

TICK WHICH MAY REQUIRE ADDITIONAL ASSESSMENT TO BE DONE.

MANUAL

HANDLING

NOISE

COSHH

Method

Statement

OTHER

CIRCULATION OF RISK ASSESSMENT:

Tick Box

Contact and Emergency Numbers
Safety Department 

Site File
Brief operatives on assessments 
Revision

ON-SITE ASSESSMENT SIGNED:                                                        Date:

POSITION:


	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Laying of Block Paviors 
	Ref: DGC_RA_0027

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:
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	Sign:
	Date:
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	Sign:
	Date:
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	Sign:
	Date:
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	Sign:
	Date:
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	Sign:
	Date:
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	Sign:
	Date:
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	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:
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	Activity: Laying of Block Paviors 
	Ref: DGC_RA_0027

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
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	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:
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	Date:

	Name:
	Sign:
	Date:
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	Date:
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	Date:
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	HEALTH & SAFETY RISK ASSESSMENT 

	Activity: Laying of Block Paviors 
	Ref: DGC_RA_0027

	I have read and understood and agree to work in accordance with the above control measures

	Name: 
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:
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	Sign:
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	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:

	Name:
	Sign:
	Date:


Likelihood





Severity
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